TN-O-G0017

Line of Sight Sensitivity Equations

Eugene Huang

April 20, 1992

GEMINI PROJECT OFFICE 950 N. Cherry Ave. Tucson, Arizona 85719 Phone: (602) 325-9329 Fax: (602) 322-8590

LINE OF SIGHT SENSITIVITY EQUATIONS

1.0 Introduction

The intent of this report is to document the line of sight sensitivity equations for a Cassegrain telescope. These equations express the image motions at the focal plane in terms of the motions of primary, secondary, and focal plane. A numerical example is given for the Gemini F/16 IR configuration. The results are checked against those obtained from Code V computer software for the same optical configuration.

2.0 Derivation of Equations

Figure 1 shows the location of the optical elements in a Cassegrain telescope together with the sign convention for their motions in a right hand cartesian coordinate system. The line of sight sensitivity equations are obtained from the following effects to the image motions:

1. Rotation of the primary, Rp, relative to optical axis will cause image motion of twice the angle Rp.

2. Rotation of the secondary, Rs, relative to optical axis will cause image motion of - 2 A Rs /L; where L is the system focal length and A is the distance between the secondary and focal plane.

3. Rotation of the focal plane will cause no image motion.

4. Translation of the focal plane, Tf , relative to optical axis will cause image motion the same amount with negative sign.

5. The rigid body rotation relative to optical axis will cause image motion of the same angle. 6. The rigid body translation will cause no image motion.

Based on the effects 1 through 4, the image motion about Y axis can be expressed by:

y y y x x x Ri = 2 Rp - ( 2 A / L ) Rs - ( 1 / L ) Tf + C1 Tp + C2 Ts (1)

Here the sensitivity factors C1 and C2 for the translations of the primary and secondary can be obtained from the effects 5 and 6 as follows.

For a unit rigid body rotation about primary, equation (1) yields:

1 = 2 - 2 A / L + B / L + C2 ( A - B ) Here B is the distance between the primary and focal plane. And this gives the sensitivity factor C2 :

Line of Sight Sensitivity Equations TN-O-G0017

C2 = 1 / L - ( 1 - A / L ) / ( A - B ) = 1 / L - 1 / Lp

Here Lp is the primary focal length which is related to the system focal length by ( see figure 1) :

L = A Lp / H = A Lp / ( Lp + B - A )

For a unit rigid body translation, equation (1) yieds :

0 = - 1 / L + C1 + C2

Hence

C1 = 1 / L - C2 = 1 / Lp

Therefore the image motion about Y axis is :

y y y x x x

Ri = 2 Rp - ( 2 A / L ) Rs + ( 1 / Lp ) Tp - ( 1 / Lp - 1 / L ) Ts - ( 1 / L ) Tf (2)

Similarly the image motion about X axis is obtained as :

x x x y y y

Ri = - 2 Rp + ( 2 A / L ) Rs + ( 1 / Lp ) Tp - ( 1 / Lp - 1 / L ) Ts - ( 1 / L ) Tf (3)

3.0 Example

Gemini F/16 IR configuration has L = 128 m , Lp = 14.4 m , and A = 16.539 m. The line of sight sensitivity equations (2) and (3) give :

y y y x x x

Ri = 2.0 Rp - 0.2584 Rs + 0.0694 Tp - 0.0616 Ts - 0.0078 Tf x x x y y y

Ri = - 2.0 Rp + 0.2584 Rs + 0.0694 Tp - 0.0616 Ts - 0.0078Tf or x y y y x x x

Ti = L Ri = 256.0 Rp - 33.078 Rs + 8.8888 Tp - 7.8888 Ts - Tf y x x x y y y

Ti = L Ri = - 256.0 Rp + 33.078 Rs + 8.8888 Tp - 7.8888 Ts - Tf x y

Line of Sight Sensitivity Equations TN-O-G0017

Page 2

Here Ti is the image motion at focal plane along X axis and Ti is the image motion at focal plane along Y axis.

Table 1 shows the optical sensitivity obtained from Code V for the F/16 IR configuration. This data are consistent with the results obtained above.

Table 1 LINE OF SIGHT SENSITIVITY FOR GEMINI F/16 IR CONFIGURATION

IMAGE MOTION AT FOCAL PLANE (mm) DISPLACEMENT PRIMARY SECONDARY FOCAL PLANE x y x y x y Ti Ti Ti Ti Ti Ti Tx = 0.025 mm 0.22222 0.0 - 0.19722 0.0 -0.025 0.0 Ty = 0.025 mm 0.0 0.22222 0.0 - 0.19722 0.0 - 0.025 Tz = 0.025 mm 0.0 0.0 0.0 0.0 0.0 0.0 Rx = 0.0005 degree 0.0 - 2.23402 0.0 0.28867 0.0 0.0 Ry = 0.0005 degree 2.23402 0.0 - 0.28867 0.0 0.0 0.0 Rz = 0.0005 degree 0.0 0.0 0.0 0.0 0.0 0.0

Line of Sight Sensitivity Equations TN-O-G0017